// Arduino Nano Every LED Blink

void setup() {
  pinMode(LED_BUILTIN, OUTPUT);
}

void loop() {
  digitalWrite(LED_BUILTIN, HIGH); // Turn LED on
  delay(2000);                     // Wait 1 second

  digitalWrite(LED_BUILTIN, LOW);  // Turn LED off
  delay(1000);                     // Wait 1 second
}